apple-history.com / Mac mini Server (Mid 2010)

apple-history / Mac mini Server (Mid 2010)

# Mac mini Server (Mid 2010)

Essentials

Family: Servers

Codename: ?

Gestalt ID: 406

Minimum OS: 10.6.4

Maximum OS: 10.10.4

Introduced: June 2010

Terminated: July 2011

Processor

CPU: Intel Mobile Core 2 Duo (P7xxx/P8xxx)

CPU Speed: 2.66 GHz

CPU Cores: 2

FPU: integrated

Bus Speed: 1066 MHz

Register Width: 64-bit

Data Bus Width: 64-bit

Address Bus Width: 64-bit

Level 1 Cache: 32 kB data, 32 kB instruction

Level 2 Cache: 3 MB on-processor

ROM: EFI

RAM Type: PC3-8500 DDR3 SDRAM

Minimum RAM Speed: 1066 MHz

Onboard RAM: 0 MB

RAM slots: 2

Maximum RAM: 8 GB

Expansion Slots: SDXC card

Video

GPU: NVIDIA GeForce 320M

VRAM: 256 MB shared (see notes)

Max Resolution: 1920x1200 via HDMI, 2560x1600 via Mini Displayport

Video Out: HDMI, Mini DisplayPort

Storage

Hard Drive: 2x 500GB 5400 RPM

ATA Bus: Serial ATA

Input/Output

USB: 4 (2.0)

Firewire800: 1

Audio Out: stereo 24 bit mini, Optical S/PDIF, HDMI, HDMI via Mini DisplayPort

Audio In: stereo 24 bit mini, Optical S/PDIF

Speaker: mono

Networking

Ethernet: 10/100/1000Base-T

Wi-Fi: 802.11a/b/g/n

Bluetooth: 4.0

Miscellaneous

Power: 85 Watts

Dimensions: 1.4" H x 7.7" W x 7.7" D

Weight: 3.0 lbs.

Notes

The Mac mini's graphics chipset used a portion of main memory as VRAM. Though reported as a 256 MB graphics system, this was actually a minimum. Actual usage varied with graphics load, resulting in slightly less RAM available for system use.

Introduced in June 2010, the Mac mini Server (Mid 2010) came with an unlimited license for Max OS X Server Snow Leopard. It was housed in the same case size and shape as its contemporary Mac mini Mac mini (Mid 2010), but without an optical drive, which was removed to accommodate a second hard drive. It shipped in a single configuration, with a 2.66 GHz Dual-core processor, 4 GB of RAM, and two 500 GB hard drives, for $999.

Picture Credits:
Apple, Inc.