apple-history.com / Power Macintosh 5200 LC

apple-history / Power Macintosh 5200 LC

# Power Macintosh 5200 LC

AKA

Performa 5200CD

Performa 5210CD

Performa 5215CD

Performa 5220CD

Essentials

Family: Macintosh LC

Codename: Trailblazer, Bongo, Rebound, Transformer

Gestalt ID: 41

Minimum OS: 7.5.1

Maximum OS: 9.1

Introduced: April 1995

Terminated: April 1996

Processor

CPU: PowerPC 603

CPU Speed: 75 MHz

FPU: integrated

Bus Speed: 37.5 MHz

Register Width: 32-bit

Data Bus Width: 64-bit

Address Bus Width: 32-bit

Level 1 Cache: 8 kB data, 8 kB instruction

Level 2 Cache: 256 kB

ROM: 4 MB

RAM Type: 72 pin SIMM

Minimum RAM Speed: 80 ns

Onboard RAM: 0 MB

RAM slots: 2

Maximum RAM: 64 MB

Expansion Slots: 1 LC PDS, comm, video i/o, TV

Video

Monitor: 15" CRT (built-in)

VRAM: 1 MB

Max Resolution: 832x624

Storage

Hard Drive: 500 MB

ATA Bus: IDE

Floppy Drive: 1.4 MB SuperDrive

Optical Drive: 4x CD-ROM

Input/Output

ADB: 1

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: stereo 16 bit mini

Audio In: mono 16 bit mini

Speaker: stereo

Microphone: mono

Miscellaneous

Power: 125 Watts

Dimensions: 17.5" H x 15.1" W x 16" D

Weight: 47 lbs.

Introduced in April 1995, The 5200 LC was the first LC model with a PowerPC chip. Released initially only in educational markets, the 5200 LC was powered by a 75 MHz 603 processor, a lower voltage variant of the 601, and came in a restyled LC 550 all-in-one case. It sold for $2000, and was replaced in April 1996 by the faster 5260. The 5200 was also released in Apple's Performa line as the Performas 5200CD, 5210CD, 5215CD, and 5220CD, each of which had different hardware and software bundles.

Picture Credits:
John Greenleigh/Flipside Studios