Previous 0.5, compiled on:  Jun 10 2014, 16:05:13
Forcing RTC checksum to 32 8d
Loading SCSI disks:
SCSI Disk0: C:\Documents and Settings\Administrator\Desktop\New Folder\Copy of ns08.dd
SCSI Disk1: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk2: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk3: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk4: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk5: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk6: C:\Documents and Settings\Administrator\Desktop\next
Loading magneto-optical disks:
MO Disk0: C:\Documents and Settings\Administrator\Desktop\next
MO Disk1: C:\Documents and Settings\Administrator\Desktop\next
SCC: Device Reset
Forcing RTC checksum to 32 8d
Loading SCSI disks:
SCSI Disk0: C:\Documents and Settings\Administrator\Desktop\New Folder\Copy of ns08.dd
SCSI Disk1: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk2: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk3: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk4: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk5: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk6: C:\Documents and Settings\Administrator\Desktop\next
Loading magneto-optical disks:
MO Disk0: C:\Documents and Settings\Administrator\Desktop\next
MO Disk1: C:\Documents and Settings\Administrator\Desktop\next
SCC: Device Reset
Host system has accurate delays. (2)
SID read at $0200c800 PC=$00000028
SCR1 read at $0200c000 PC=$00000050
SCR1 read at $0200c001 PC=$00000050
SCR1 read at $0200c002 PC=$00000050
SCR1 read at $0200c003 PC=$00000050
IO write at $02006010 val=31 PC=$0000007c
IO write at $02006011 val=38 PC=$0000007c
IO write at $02006012 val=68 PC=$0000007c
IO write at $02006013 val=0d PC=$0000007c
IO write at $02006014 val=00 PC=$0000007c
Interrupt mask: 00000000
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[RTC] reading val $94 from addr $00 at PC=$000063c0
[RTC] reading val $0F from addr $01 at PC=$000063c0
[RTC] reading val $40 from addr $02 at PC=$000063c0
[RTC] reading val $00 from addr $03 at PC=$000063c0
[RTC] reading val $00 from addr $04 at PC=$000063c0
[RTC] reading val $00 from addr $05 at PC=$000063c0
[RTC] reading val $0F from addr $06 at PC=$000063c0
[RTC] reading val $00 from addr $07 at PC=$000063c0
[RTC] reading val $30 from addr $08 at PC=$000063c0
[RTC] reading val $90 from addr $09 at PC=$000063c0
[RTC] reading val $FB from addr $0A at PC=$000063c0
[RTC] reading val $6D from addr $0B at PC=$000063c0
[RTC] reading val $00 from addr $0C at PC=$000063c0
[RTC] reading val $00 from addr $0D at PC=$000063c0
[RTC] reading val $4B from addr $0E at PC=$000063c0
[RTC] reading val $00 from addr $0F at PC=$000063c0
[RTC] reading val $00 from addr $10 at PC=$000063c0
[RTC] reading val $00 from addr $11 at PC=$000063c0
[RTC] reading val $73 from addr $12 at PC=$000063c0
[RTC] reading val $64 from addr $13 at PC=$000063c0
[RTC] reading val $00 from addr $14 at PC=$000063c0
[RTC] reading val $00 from addr $15 at PC=$000063c0
[RTC] reading val $00 from addr $16 at PC=$000063c0
[RTC] reading val $00 from addr $17 at PC=$000063c0
[RTC] reading val $00 from addr $18 at PC=$000063c0
[RTC] reading val $00 from addr $19 at PC=$000063c0
[RTC] reading val $00 from addr $1A at PC=$000063c0
[RTC] reading val $00 from addr $1B at PC=$000063c0
[RTC] reading val $00 from addr $1C at PC=$000063c0
[RTC] reading val $00 from addr $1D at PC=$000063c0
[RTC] reading val $32 from addr $1E at PC=$000063c0
[RTC] reading val $8D from addr $1F at PC=$000063c0
[RTC] reading val $94 from addr $00 at PC=$000063c0
[RTC] reading val $0F from addr $01 at PC=$000063c0
[RTC] reading val $40 from addr $02 at PC=$000063c0
[RTC] reading val $00 from addr $03 at PC=$000063c0
[RTC] reading val $00 from addr $04 at PC=$000063c0
[RTC] reading val $00 from addr $05 at PC=$000063c0
[RTC] reading val $0F from addr $06 at PC=$000063c0
[RTC] reading val $00 from addr $07 at PC=$000063c0
[RTC] reading val $30 from addr $08 at PC=$000063c0
[RTC] reading val $90 from addr $09 at PC=$000063c0
[RTC] reading val $FB from addr $0A at PC=$000063c0
[RTC] reading val $6D from addr $0B at PC=$000063c0
[RTC] reading val $00 from addr $0C at PC=$000063c0
[RTC] reading val $00 from addr $0D at PC=$000063c0
[RTC] reading val $4B from addr $0E at PC=$000063c0
[RTC] reading val $00 from addr $0F at PC=$000063c0
[RTC] reading val $00 from addr $10 at PC=$000063c0
[RTC] reading val $00 from addr $11 at PC=$000063c0
[RTC] reading val $73 from addr $12 at PC=$000063c0
[RTC] reading val $64 from addr $13 at PC=$000063c0
[RTC] reading val $00 from addr $14 at PC=$000063c0
[RTC] reading val $00 from addr $15 at PC=$000063c0
[RTC] reading val $00 from addr $16 at PC=$000063c0
[RTC] reading val $00 from addr $17 at PC=$000063c0
[RTC] reading val $00 from addr $18 at PC=$000063c0
[RTC] reading val $00 from addr $19 at PC=$000063c0
[RTC] reading val $00 from addr $1A at PC=$000063c0
[RTC] reading val $00 from addr $1B at PC=$000063c0
[RTC] reading val $00 from addr $1C at PC=$000063c0
[RTC] reading val $00 from addr $1D at PC=$000063c0
[RTC] reading val $32 from addr $1E at PC=$000063c0
[RTC] reading val $8D from addr $1F at PC=$000063c0
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
IO write at $02010000 val=50 PC=$00000970
[KMS] Device 1 disabled (mask: 00000000)
[RTC] reading val $94 from addr $00 at PC=$000063c0
[RTC] reading val $0F from addr $01 at PC=$000063c0
[RTC] reading val $40 from addr $02 at PC=$000063c0
[RTC] reading val $00 from addr $03 at PC=$000063c0
[RTC] reading val $00 from addr $04 at PC=$000063c0
[RTC] reading val $00 from addr $05 at PC=$000063c0
[RTC] reading val $0F from addr $06 at PC=$000063c0
[RTC] reading val $00 from addr $07 at PC=$000063c0
[RTC] reading val $30 from addr $08 at PC=$000063c0
[RTC] reading val $90 from addr $09 at PC=$000063c0
[RTC] reading val $FB from addr $0A at PC=$000063c0
[RTC] reading val $6D from addr $0B at PC=$000063c0
[RTC] reading val $00 from addr $0C at PC=$000063c0
[KMS] Device 1 disabled (mask: 00000000)
[RTC] reading val $00 from addr $0D at PC=$000063c0
[RTC] reading val $4B from addr $0E at PC=$000063c0
[RTC] reading val $00 from addr $0F at PC=$000063c0
[RTC] reading val $00 from addr $10 at PC=$000063c0
[RTC] reading val $00 from addr $11 at PC=$000063c0
[RTC] reading val $73 from addr $12 at PC=$000063c0
[RTC] reading val $64 from addr $13 at PC=$000063c0
[RTC] reading val $00 from addr $14 at PC=$000063c0
[RTC] reading val $00 from addr $15 at PC=$000063c0
[RTC] reading val $00 from addr $16 at PC=$000063c0
[RTC] reading val $00 from addr $17 at PC=$000063c0
[RTC] reading val $00 from addr $18 at PC=$000063c0
[RTC] reading val $00 from addr $19 at PC=$000063c0
[RTC] reading val $00 from addr $1A at PC=$000063c0
[RTC] reading val $00 from addr $1B at PC=$000063c0
[RTC] reading val $00 from addr $1C at PC=$000063c0
[RTC] reading val $00 from addr $1D at PC=$000063c0
[RTC] reading val $32 from addr $1E at PC=$000063c0
[RTC] reading val $8D from addr $1F at PC=$000063c0
SCR1 read at $0200c000 PC=$00000c36
SCR1 read at $0200c001 PC=$00000c36
SCR1 read at $0200c002 PC=$00000c36
SCR1 read at $0200c003 PC=$00000c36
[KMS] Access keyboard/mouse register
[KMS] Data = EF000000
Keyboard/Mouse: Set address to 0
[KMS] Access keyboard/mouse register
[KMS] Data = 00030000
Writing keyboard 0, register 0
Turn on keyboard LED1
Turn on keyboard LED2
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Access keyboard/mouse register
[KMS] Data = 00000000
Writing keyboard 0, register 0
Turn off keyboard LED1
Turn off keyboard LED2
SCC A, Reg0 read: ff
SCC A, Reg9 write: ca
SCC: Device Reset
SCC A, Reg4 write: 44
SCC A, Reg11 write: 50
SCC A, Reg14 write: 10
SCC A, Reg12 write: 0a
SCC A, Reg13 write: 00
SCC A, Reg14 write: 11
SCC A, Reg10 write: 00
SCC A, Reg3 write: c1
SCC A, Reg5 write: ea
SCC A, Reg15 write: 00
SCC B, Reg15 read: 00
SCC B, Reg4 write: 44
SCC B, Reg11 write: 50
SCC B, Reg14 write: 10
SCC B, Reg12 write: 0a
SCC B, Reg13 write: 00
SCC B, Reg14 write: 11
SCC B, Reg10 write: 00
SCC B, Reg3 write: c1
SCC B, Reg5 write: ea
SCC B, Reg15 write: 00
Interrupt mask: 00200000
SCC A, Reg15 read: 00
SCC A, Reg1 write: 40
SCC A, Reg1 read: 00
SCC A, Reg1 write: c0
SCC A, Reg0 read: 01
SCC A, Data read: 40
SCC A, Reg0 read: 01
SCC A, Reg1 write: 00
Interrupt mask: 00000000
SCC A, Reg1 read: 00
SCC A, Reg1 write: 00
SCC B, Reg1 read: 00
SCC B, Reg0 read: ff
SCC B, Data write: 40
SCC B, Reg0 read: 05
SCC B, Data read: 40
[EN] Reset write at $02006006 val=$80 PC=$00006842
[EN] Transmitter masks write at $02006001 val=$00 PC=$00006848
[EN] Receiver masks write at $02006003 val=$00 PC=$0000684c
[EN] Transmitter status write at $02006000 val=$ff PC=$00006850
[EN] Receiver status write at $02006002 val=$ff PC=$00006852
[EN] Transmitter mode write at $02006004 val=$02 PC=$00006856
[EN] Receiver mode write at $02006005 val=$00 PC=$0000685c
[EN] MAC byte 0 write at $02006008 val=$00 PC=$00005eb8
[EN] MAC byte 1 write at $02006009 val=$00 PC=$00005eb8
[EN] MAC byte 2 write at $0200600a val=$0f PC=$00005eb8
[EN] MAC byte 3 write at $0200600b val=$00 PC=$00005eb8
[EN] MAC byte 4 write at $0200600c val=$30 PC=$00005ec6
[EN] MAC byte 5 write at $0200600d val=$90 PC=$00005ec6
[EN] Receiver mode write at $02006005 val=$06 PC=$00006ce6
Interrupt mask: 08000000
[EN] Reset write at $02006006 val=$00 PC=$00006906
Starting Ethernet Transmitter/Receiver
[EN] Transmitter mode read at $02006004 val=$02 PC=$00002d9c
[EN] Transmitter mode write at $02006004 val=$00 PC=$00002d9c
[EN] Transmitter status read at $02006000 val=$80 PC=$00006a7a
[EN] Sending packet to 00:00:0F:00:30:90
[EN] Receiving packet from 00:00:0F:00:30:90
[EN] Receiving packet: Transfer complete.
[EN] Receiver status read at $02006002 val=$80 PC=$00006b72
[EN] Receiver status write at $02006002 val=$ff PC=$00006b84
[EN] Receiver mode write at $02006005 val=$06 PC=$00006ce6
[EN] MAC byte 5 write at $0200600d val=$91 PC=$00002ea0
[EN] Transmitter status read at $02006000 val=$a0 PC=$00006a7a
[EN] Sending packet to 00:00:0F:00:30:90
[EN] Transmitter status read at $02006000 val=$a0 PC=$00006a7a
[EN] Sending packet to FF:FF:FF:FF:FF:FF
[EN] Receiving packet from 00:00:0F:00:30:90
[EN] Receiving packet: Transfer complete.
[EN] Receiver status read at $02006002 val=$80 PC=$00006b72
[EN] Receiver status write at $02006002 val=$ff PC=$00006b84
[EN] Receiver mode write at $02006005 val=$06 PC=$00006ce6
[EN] Transmitter mode write at $02006004 val=$02 PC=$00002f76
[EN] Reset write at $02006006 val=$80 PC=$00006b02
Stopping Ethernet Transmitter/Receiver
[RTC] writing val $00 to addr $B2 at PC=$00006302
[RTC] writing val $B0 to addr $B1 at PC=$00006302
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $04 from addr $20 at PC=$000063c0
[RTC] reading val $05 from addr $20 at PC=$000063c0
Interrupt mask: 20000000
Interrupt mask: 08000000
Interrupt mask: 00800000
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Sound out command:
[KMS] Sound out enable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
Interrupt mask: 08000000
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
ESP Command: Illegal command!
Interrupt mask: 00000000
SCC A, Reg9 write: c0
SCC: Device Reset
SCC A, Reg9 write: 02
SCC A, Reg11 write: 50
SCC A, Reg48 write: 10
SCC A, Reg4 write: 44
SCC A, Reg3 write: c0
SCC A, Reg5 write: 60
SCC A, Reg14 write: 00
IO write at $02018004 val=00 PC=$00006570
Bus error $02018005 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 419
Bus error $02018006 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 409
Bus error $02018007 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 419
SCC A, Reg12 write: 0a
SCC A, Reg13 write: 00
SCC A, Reg14 write: 02
SCC A, Reg14 write: 03
SCC A, Reg3 write: c1
SCC A, Reg5 write: ea
SCC B, Reg9 write: 02
SCC B, Reg11 write: 50
SCC B, Reg48 write: 10
SCC B, Reg4 write: 44
SCC B, Reg3 write: c0
SCC B, Reg5 write: 60
SCC B, Reg14 write: 00
IO write at $02018004 val=00 PC=$00006570
Bus error $02018005 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 419
Bus error $02018006 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 409
Bus error $02018007 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 419
SCC B, Reg12 write: 0a
SCC B, Reg13 write: 00
SCC B, Reg14 write: 02
SCC B, Reg14 write: 03
SCC B, Reg3 write: c1
SCC B, Reg5 write: ea
[RTC] writing val $00 to addr $B2 at PC=$00006302
[EN] Reset write at $02006006 val=$80 PC=$00001242
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($07FFC178).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($07FFC148).
Key pressed: left alt
Keycode: $00, Modifiers: $00
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($0410FE88).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($0410FE58).
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($0410E174).
[DMA] Channel SCSI: 12 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($0410FE5C).
Key released: left alt
Keycode: $00, Modkeys: $00
SCR1 read at $0200c000 PC=$0404a4c8
SCR1 read at $0200c001 PC=$0404a4c8
SCR1 read at $0200c002 PC=$0404a4c8
SCR1 read at $0200c003 PC=$0404a4c8
Interrupt mask: 00000000
[RTC] writing val $00 to addr $B2 at PC=$04047fa2
[RTC] reading val $00 from addr $30 at PC=$040480c2
[KMS] Access keyboard/mouse register
[KMS] Data = EF000000
Keyboard/Mouse: Set address to 0
[KMS] Access keyboard/mouse register
[KMS] Data = 00000000
Writing keyboard 0, register 0
Turn off keyboard LED1
Turn off keyboard LED2
Interrupt mask: 00000004
Interrupt mask: 80000004
Interrupt mask: 8000000c
[RTC] reading val $00 from addr $30 at PC=$040480c2
[RTC] writing val $00 to addr $B2 at PC=$04047fa2
Interrupt mask: 8001800f
SCC A, Reg5 write: 02
SCC B, Reg5 write: 02
SCR1 read at $0200c000 PC=$0405a108
SCR1 read at $0200c001 PC=$0405a108
SCR1 read at $0200c002 PC=$0405a108
SCR1 read at $0200c003 PC=$0405a108
Interrupt mask: 8201800f
Interrupt mask: 8201a00f
Interrupt mask: 8201a00f
ESP FIFO read: FIFO is empty!
Interrupt mask: 8601a00f
Interrupt mask: 8601b00f
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758C8).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758C8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[EN] MAC byte 0 write at $02006008 val=$00 PC=$040485a0
[EN] MAC byte 1 write at $02006009 val=$00 PC=$040485a0
[EN] MAC byte 2 write at $0200600a val=$0f PC=$040485a0
[EN] MAC byte 3 write at $0200600b val=$00 PC=$040485a0
[EN] MAC byte 4 write at $0200600c val=$30 PC=$040485ae
[EN] MAC byte 5 write at $0200600d val=$90 PC=$040485ae
[DSP] write val -2147483648 PC=40522f4 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
[DSP] write val 33554432 PC=40522f8 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
[DSP] write val 0 PC=405230a C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
IO read at $0200f003 PC=$04058fc6
IO read at $0200f002 PC=$04059002
IO write at $0200f002 val=00 PC=$04059002
Interrupt mask: 8701b00f
Interrupt mask: 8701b80f
[KMS] Sound in command
[KMS] Sound in disable.
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Access volume control logic
[KMS] Data = 000000FF
Interrupt mask: 8781b80f
Interrupt mask: 87c1b80f
Interrupt mask: 87c1b90f
Interrupt mask: a7c1b90f
[RTC] reading val $00 from addr $30 at PC=$040480c2
[RTC] reading val $14 from addr $26 at PC=$040480c2
[RTC] reading val $06 from addr $25 at PC=$040480c2
[RTC] reading val $14 from addr $26 at PC=$040480c2
[RTC] reading val $19 from addr $24 at PC=$040480c2
[RTC] reading val $06 from addr $25 at PC=$040480c2
[RTC] reading val $20 from addr $22 at PC=$040480c2
[RTC] reading val $19 from addr $24 at PC=$040480c2
[RTC] reading val $51 from addr $21 at PC=$040480c2
[RTC] reading val $20 from addr $22 at PC=$040480c2
[RTC] reading val $08 from addr $20 at PC=$040480c2
[RTC] reading val $51 from addr $21 at PC=$040480c2
[RTC] writing val $30 to addr $B1 at PC=$04047fa2
[RTC] writing val $27 to addr $A0 at PC=$04047fa2
setting 0 to 1b
Offset is 1403225469
[RTC] writing val $52 to addr $A1 at PC=$04047fa2
setting 1 to 34
Offset is 1403225469
[RTC] writing val $07 to addr $A2 at PC=$04047fa2
setting 2 to 7
Offset is 1403225469
[RTC] writing val $01 to addr $A3 at PC=$04047fa2
[RTC] writing val $07 to addr $A4 at PC=$04047fa2
setting 3 to 7
Offset is 1403225469
[RTC] writing val $10 to addr $A5 at PC=$04047fa2
setting 4 to a
Offset is 1403225469
[RTC] writing val $97 to addr $A6 at PC=$04047fa2
setting 5 to 61
Offset is 526996721
[RTC] writing val $B0 to addr $B1 at PC=$04047fa2
[RTC] reading val $00 from addr $30 at PC=$040480c2
[RTC] reading val $31 from addr $26 at PC=$040480c2
[RTC] reading val $03 from addr $25 at PC=$040480c2
[RTC] reading val $31 from addr $26 at PC=$040480c2
[RTC] reading val $02 from addr $24 at PC=$040480c2
[RTC] reading val $03 from addr $25 at PC=$040480c2
[RTC] reading val $07 from addr $22 at PC=$040480c2
[RTC] reading val $02 from addr $24 at PC=$040480c2
[RTC] reading val $50 from addr $21 at PC=$040480c2
[RTC] reading val $07 from addr $22 at PC=$040480c2
[RTC] reading val $03 from addr $20 at PC=$040480c2
[RTC] reading val $50 from addr $21 at PC=$040480c2
[RTC] reading val $00 from addr $30 at PC=$040480c2
[RTC] reading val $31 from addr $26 at PC=$040480c2
[RTC] reading val $03 from addr $25 at PC=$040480c2
[RTC] reading val $31 from addr $26 at PC=$040480c2
[RTC] reading val $02 from addr $24 at PC=$040480c2
[RTC] reading val $03 from addr $25 at PC=$040480c2
[RTC] reading val $07 from addr $22 at PC=$040480c2
[RTC] reading val $02 from addr $24 at PC=$040480c2
[RTC] reading val $50 from addr $21 at PC=$040480c2
[RTC] reading val $07 from addr $22 at PC=$040480c2
[RTC] reading val $03 from addr $20 at PC=$040480c2
[RTC] reading val $50 from addr $21 at PC=$040480c2
[RTC] reading val $00 from addr $30 at PC=$040480c2
[RTC] reading val $31 from addr $26 at PC=$040480c2
[RTC] reading val $03 from addr $25 at PC=$040480c2
[RTC] reading val $31 from addr $26 at PC=$040480c2
[RTC] reading val $02 from addr $24 at PC=$040480c2
[RTC] reading val $03 from addr $25 at PC=$040480c2
[RTC] reading val $07 from addr $22 at PC=$040480c2
[RTC] reading val $02 from addr $24 at PC=$040480c2
[RTC] reading val $50 from addr $21 at PC=$040480c2
[RTC] reading val $07 from addr $22 at PC=$040480c2
[RTC] reading val $18 from addr $20 at PC=$040480c2
[RTC] reading val $50 from addr $21 at PC=$040480c2
[RTC] reading val $94 from addr $00 at PC=$000063c0
[RTC] reading val $0F from addr $01 at PC=$000063c0
[RTC] reading val $40 from addr $02 at PC=$000063c0
[RTC] reading val $00 from addr $03 at PC=$000063c0
[RTC] reading val $00 from addr $04 at PC=$000063c0
[RTC] reading val $00 from addr $05 at PC=$000063c0
[RTC] reading val $0F from addr $06 at PC=$000063c0
[RTC] reading val $00 from addr $07 at PC=$000063c0
[RTC] reading val $30 from addr $08 at PC=$000063c0
[RTC] reading val $90 from addr $09 at PC=$000063c0
[RTC] reading val $FB from addr $0A at PC=$000063c0
[RTC] reading val $6D from addr $0B at PC=$000063c0
[RTC] reading val $00 from addr $0C at PC=$000063c0
[RTC] reading val $00 from addr $0D at PC=$000063c0
[RTC] reading val $4B from addr $0E at PC=$000063c0
[RTC] reading val $00 from addr $0F at PC=$000063c0
[RTC] reading val $00 from addr $10 at PC=$000063c0
[RTC] reading val $00 from addr $11 at PC=$000063c0
[RTC] reading val $73 from addr $12 at PC=$000063c0
[RTC] reading val $64 from addr $13 at PC=$000063c0
[RTC] reading val $00 from addr $14 at PC=$000063c0
[RTC] reading val $00 from addr $15 at PC=$000063c0
[RTC] reading val $00 from addr $16 at PC=$000063c0
[RTC] reading val $00 from addr $17 at PC=$000063c0
[RTC] reading val $00 from addr $18 at PC=$000063c0
[RTC] reading val $00 from addr $19 at PC=$000063c0
[RTC] reading val $00 from addr $1A at PC=$000063c0
[RTC] reading val $00 from addr $1B at PC=$000063c0
[RTC] reading val $00 from addr $1C at PC=$000063c0
[RTC] reading val $00 from addr $1D at PC=$000063c0
[RTC] reading val $32 from addr $1E at PC=$000063c0
[RTC] reading val $8D from addr $1F at PC=$000063c0
IO write at $02010000 val=50 PC=$0000132c
Interrupt mask: 00000000
SCC A, Reg9 write: c0
SCC: Device Reset
SCC A, Reg9 write: 02
SCC A, Reg11 write: 50
SCC A, Reg48 write: 10
SCC A, Reg4 write: 44
SCC A, Reg3 write: c0
SCC A, Reg5 write: 60
SCC A, Reg14 write: 00
IO write at $02018004 val=00 PC=$00006570
Bus error $02018005 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 419
Bus error $02018006 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 409
Bus error $02018007 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 419
SCC A, Reg12 write: 0a
SCC A, Reg13 write: 00
SCC A, Reg14 write: 02
SCC A, Reg14 write: 03
SCC A, Reg3 write: c1
SCC A, Reg5 write: ea
SCC B, Reg9 write: 02
SCC B, Reg11 write: 50
SCC B, Reg48 write: 10
SCC B, Reg4 write: 44
SCC B, Reg3 write: c0
SCC B, Reg5 write: 60
SCC B, Reg14 write: 00
IO write at $02018004 val=00 PC=$00006570
Bus error $02018005 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 419
Bus error $02018006 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 409
Bus error $02018007 PC=$00006570 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMem.c at 419
SCC B, Reg12 write: 0a
SCC B, Reg13 write: 00
SCC B, Reg14 write: 02
SCC B, Reg14 write: 03
SCC B, Reg3 write: c1
SCC B, Reg5 write: ea
[RTC] writing val $00 to addr $B2 at PC=$00006302
[EN] Reset write at $02006006 val=$80 PC=$00001242
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($07FFC178).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($07FFC148).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($0410FE88).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($0410FE58).
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($0410E174).
[DMA] Channel SCSI: 12 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($0410FE5C).
SCR1 read at $0200c000 PC=$0404a4c8
SCR1 read at $0200c001 PC=$0404a4c8
SCR1 read at $0200c002 PC=$0404a4c8
SCR1 read at $0200c003 PC=$0404a4c8
Interrupt mask: 00000000
[RTC] writing val $00 to addr $B2 at PC=$04047fa2
[RTC] reading val $00 from addr $30 at PC=$040480c2
[KMS] Access keyboard/mouse register
[KMS] Data = EF000000
Keyboard/Mouse: Set address to 0
[KMS] Access keyboard/mouse register
[KMS] Data = 00000000
Writing keyboard 0, register 0
Turn off keyboard LED1
Turn off keyboard LED2
Interrupt mask: 00000004
Interrupt mask: 80000004
Interrupt mask: 8000000c
[RTC] reading val $00 from addr $30 at PC=$040480c2
[RTC] writing val $00 to addr $B2 at PC=$04047fa2
Interrupt mask: 8001800f
SCC A, Reg5 write: 02
SCC B, Reg5 write: 02
SCR1 read at $0200c000 PC=$0405a108
SCR1 read at $0200c001 PC=$0405a108
SCR1 read at $0200c002 PC=$0405a108
SCR1 read at $0200c003 PC=$0405a108
Interrupt mask: 8201800f
Interrupt mask: 8201a00f
Interrupt mask: 8201a00f
ESP FIFO read: FIFO is empty!
Interrupt mask: 8601a00f
Interrupt mask: 8601b00f
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758C8).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758C8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040758F8).
[EN] MAC byte 0 write at $02006008 val=$00 PC=$040485a0
[EN] MAC byte 1 write at $02006009 val=$00 PC=$040485a0
[EN] MAC byte 2 write at $0200600a val=$0f PC=$040485a0
[EN] MAC byte 3 write at $0200600b val=$00 PC=$040485a0
[EN] MAC byte 4 write at $0200600c val=$30 PC=$040485ae
[EN] MAC byte 5 write at $0200600d val=$90 PC=$040485ae
[DSP] write val -2147483648 PC=40522f4 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
[DSP] write val 33554432 PC=40522f8 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
[DSP] write val 0 PC=405230a C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
IO read at $0200f003 PC=$04058fc6
IO read at $0200f002 PC=$04059002
IO write at $0200f002 val=00 PC=$04059002
Interrupt mask: 8701b00f
Interrupt mask: 8701b80f
[KMS] Sound in command
[KMS] Sound in disable.
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Access volume control logic
[KMS] Data = 000000FF
Interrupt mask: 8781b80f
Interrupt mask: 87c1b80f
Interrupt mask: 87c1b90f
Interrupt mask: a7c1b90f
[RTC] writing val $30 to addr $B1 at PC=$04047fa2
[RTC] writing val $00 to addr $A0 at PC=$04047fa2
setting 0 to 0
Offset is 526996783
[RTC] writing val $00 to addr $A1 at PC=$04047fa2
setting 1 to 0
Offset is 526999903
[RTC] writing val $12 to addr $A2 at PC=$04047fa2
setting 2 to c
Offset is 526985503
[RTC] writing val $01 to addr $A3 at PC=$04047fa2
[RTC] writing val $02 to addr $A4 at PC=$04047fa2
setting 3 to 2
Offset is 527417503
[RTC] writing val $07 to addr $A5 at PC=$04047fa2
setting 4 to 7
Offset is 535366303
[RTC] writing val $87 to addr $A6 at PC=$04047fa2
setting 5 to 57
Offset is 850985503
[RTC] writing val $B0 to addr $B1 at PC=$04047fa2
Interrupt mask: a7c1b92f
Key pressed: right alt
Keycode: $00, Modifiers: $00
Key pressed: m
Short :2
Key released: m
Key released: right alt
Keycode: $00, Modkeys: $00
[RTC] reading val $00 from addr $30 at PC=$040480c2
[RTC] reading val $41 from addr $26 at PC=$040480c2
[RTC] reading val $06 from addr $25 at PC=$040480c2
[RTC] reading val $41 from addr $26 at PC=$040480c2
[RTC] reading val $07 from addr $24 at PC=$040480c2
[RTC] reading val $06 from addr $25 at PC=$040480c2
[RTC] reading val $05 from addr $22 at PC=$040480c2
[RTC] reading val $07 from addr $24 at PC=$040480c2
[RTC] reading val $44 from addr $21 at PC=$040480c2
[RTC] reading val $05 from addr $22 at PC=$040480c2
[RTC] reading val $28 from addr $20 at PC=$040480c2
[RTC] reading val $44 from addr $21 at PC=$040480c2
[RTC] reading val $00 from addr $30 at PC=$040480c2
[RTC] reading val $41 from addr $26 at PC=$040480c2
[RTC] reading val $06 from addr $25 at PC=$040480c2
[RTC] reading val $41 from addr $26 at PC=$040480c2
[RTC] reading val $07 from addr $24 at PC=$040480c2
[RTC] reading val $06 from addr $25 at PC=$040480c2
[RTC] reading val $05 from addr $22 at PC=$040480c2
[RTC] reading val $07 from addr $24 at PC=$040480c2
[RTC] reading val $44 from addr $21 at PC=$040480c2
[RTC] reading val $05 from addr $22 at PC=$040480c2
[RTC] reading val $30 from addr $20 at PC=$040480c2
[RTC] reading val $44 from addr $21 at PC=$040480c2
[RTC] reading val $00 from addr $30 at PC=$040480c2
[RTC] reading val $41 from addr $26 at PC=$040480c2
[RTC] reading val $06 from addr $25 at PC=$040480c2
[RTC] reading val $41 from addr $26 at PC=$040480c2
[RTC] reading val $07 from addr $24 at PC=$040480c2
[RTC] reading val $06 from addr $25 at PC=$040480c2
[RTC] reading val $05 from addr $22 at PC=$040480c2
[RTC] reading val $07 from addr $24 at PC=$040480c2
[RTC] reading val $44 from addr $21 at PC=$040480c2
[RTC] reading val $05 from addr $22 at PC=$040480c2
[RTC] reading val $36 from addr $20 at PC=$040480c2
[RTC] reading val $44 from addr $21 at PC=$040480c2
Key pressed: f10
Keycode: $58, Modifiers: $00
Interrupt mask: a7c1b92b
Key released: f10
Keycode: $58, Modkeys: $00
Interrupt mask: a7c1b92f
[RTC] reading val $00 from addr $30 at PC=$040480c2
[RTC] reading val $41 from addr $26 at PC=$040480c2
[RTC] reading val $06 from addr $25 at PC=$040480c2
[RTC] reading val $41 from addr $26 at PC=$040480c2
[RTC] reading val $07 from addr $24 at PC=$040480c2
[RTC] reading val $06 from addr $25 at PC=$040480c2
[RTC] reading val $05 from addr $22 at PC=$040480c2
[RTC] reading val $07 from addr $24 at PC=$040480c2
[RTC] reading val $45 from addr $21 at PC=$040480c2
[RTC] reading val $05 from addr $22 at PC=$040480c2
[RTC] reading val $33 from addr $20 at PC=$040480c2
[RTC] reading val $45 from addr $21 at PC=$040480c2
[RTC] writing val $40 to addr $B2 at PC=$04047fa2
[RTC] Power down!
