apple-history.com / Macintosh IIci

apple-history / Macintosh IIci
Follow @apple_history
Tweet

# Macintosh IIci

Essentials

Family: Macintosh II

Codename: Aurora II, Cobra II, Pacific, Stingray

Gestalt ID: 11

Minimum OS: 6.0.4

Maximum OS: 7.6.1

Introduced: September 1989

Terminated: February 1993

Processor

CPU: Motorola MC68030

CPU Speed: 25 MHz

FPU: 68882

Bus Speed: 25 MHz

Register Width: 32-bit

Data Bus Width: 32-bit

Address Bus Width: 32-bit

Level 1 Cache: 256 bytes data, 256 bytes instruction

Level 2 Cache: optional 32 kB

ROM: 512 kB

RAM Type: 30 pin SIMM

Minimum RAM Speed: 80 ns

Onboard RAM: 0 MB

RAM slots: 8

Maximum RAM: 128 MB

Expansion Slots: 3 NuBus

Video

VRAM: 1 MB DRAM

Max Resolution: 8 bit, 640x480

Video Out: DB-15

Storage

Hard Drive: 40-80 MB

Floppy Drive: 1.4 MB SuperDrive

Input/Output

ADB: 2

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: stereo 8 bit mini

Speaker: mono

Miscellaneous

Power: 159 Watts

Dimensions: 5.5" H x 11.9" W x 14.4" D

Weight: 13.6 lbs.

The Mac IIci was a faster version of the IIcx, and one of the more popular Macs ever. It was the first Mac to have built in color video circuitry, and the first Mac with 32-bit clean ROMs. It sold for $6,700.

Picture Credits:
AppleDesign