apple-history.com / Macintosh LC III+

apple-history / Macintosh LC III+
Follow @apple_history
Tweet

# Macintosh LC III+

AKA

Performa 460

Performa 466

Performa 467

Essentials

Family: Macintosh LC

Codename: ?

Gestalt ID: 62

Minimum OS: 7.1

Maximum OS: 7.6.1

Introduced: October 1993

Terminated: February 1994

Processor

CPU: Motorola MC68030

CPU Speed: 33 MHz

FPU: optional 68882

Bus Speed: 33 MHz

Register Width: 32-bit

Data Bus Width: 32-bit

Address Bus Width: 32-bit

Level 1 Cache: 256 bytes data, 256 bytes instruction

ROM: 1 MB

RAM Type: 72 pin SIMM

Minimum RAM Speed: 80 ns

Onboard RAM: 4 MB

RAM slots: 1

Maximum RAM: 36 MB

Expansion Slots: 1 LC III PDS

Video

VRAM: 512 kB - 768 kB (one socket)

Max Resolution: 8 bit 640x480

Video Out: DB-15

Storage

Hard Drive: 80-160 MB

Floppy Drive: 1.4 MB SuperDrive

Input/Output

ADB: 1

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: mono 8-bit mini

Audio In: mono 8-bit mini

Speaker: mono

Miscellaneous

Power: 50 Watts

Dimensions: 2.9" H x 12.2" W x 15.3" D

Weight: 8.8 lbs.

Introduced in October 1993, the LC III+ sold alongside its predecessor, the LC III. The III+ added a 33 MHz 68030 processor, was also sold as the Performas 460, 466, and 467. It was discontinued, along with the LC III, in February 1994.

Picture Credits:
Todo Apple Blog