apple-history.com / iMac (Rev. D)

apple-history / iMac (Rev. D)
Follow @apple_history
Tweet

# iMac (Rev. D)

Essentials

Family: iMac/eMac

Codename: ?

Gestalt ID: 406

Minimum OS: 8.5.1

Maximum OS: 10.3.9

Introduced: April 1999

Terminated: October 1999

Processor

CPU: PowerPC 750 "G3"

CPU Speed: 333 MHz

FPU: integrated

Bus Speed: 66 MHz

Register Width: 32-bit

Data Bus Width: 64-bit

Address Bus Width: 32-bit

Level 1 Cache: 32 kB data, 32 kB instruction

Level 2 Cache: 512 kB backside, 1:2

ROM: 1 MB ROM + 3 MB toolbox ROM loaded into RAM

RAM Type: 144 pin SO-DIMM

Minimum RAM Speed: 100 MHz

Onboard RAM: 0 MB

RAM slots: 2

Maximum RAM: 512 MB

Video

Monitor: 15"

VRAM: 6 MB SGRAM

Max Resolution: 1024x768

Storage

Hard Drive: 6 GB

ATA Bus: EIDE

Optical Drive: 24x CD-ROM

Input/Output

USB: 2

Audio Out: stereo 16 bit mini

Audio In: stereo 16 bit mini

Speaker: stereo, SRS

Microphone: mono

Networking

Modem: 56 kbps

Ethernet: 10/100Base-T

Miscellaneous

Power: 80 Watts

Dimensions: 15.8" H x 15.2" W x 17.6" D

Weight: 40 lbs.

In April 1999, Apple Replaced the Rev. C with the Rev. D iMac, bumping the processor speed to 333 MHz. All other specs were the same. The Rec. D iMac was terminated the following October.

Picture Credits:
Apple, Inc.