apple-history.com / iMac (Rev. C)

apple-history / iMac (Rev. C)
Follow @apple_history
Tweet

# iMac (Rev. C)

Essentials

Family: iMac/eMac

Codename: Lifesavers

Gestalt ID: 406

Minimum OS: 8.5

Maximum OS: 10.3.9

Introduced: January 1999

Terminated: April 1999

Processor

CPU: PowerPC 750 "G3"

CPU Speed: 266 MHz

FPU: integrated

Bus Speed: 66 MHz

Register Width: 32-bit

Data Bus Width: 64-bit

Address Bus Width: 32-bit

Level 1 Cache: 32 kB data, 32 kB instruction

Level 2 Cache: 512 kB backside, 1:2

ROM: 1 MB ROM + 3 MB toolbox ROM loaded into RAM

RAM Type: 144 pin SO-DIMM

Minimum RAM Speed: 100 MHz

Onboard RAM: 0 MB

RAM slots: 2

Maximum RAM: 256 MB

Video

Monitor: 15"

VRAM: 6 MB SGRAM

Max Resolution: 1024x768

Storage

Hard Drive: 6 GB

ATA Bus: EIDE

Optical Drive: 24x CD-ROM

Input/Output

USB: 2

Audio Out: stereo 16 bit mini

Audio In: stereo 16 bit mini

Speaker: stereo, SRS

Microphone: mono

Networking

Modem: 56 kbps

Ethernet: 10/100Base-T

Miscellaneous

Power: 80 Watts

Dimensions: 15.8" H x 15.2" W x 17.6" D

Weight: 40 lbs.

Announced in January 1999, the Rev. C iMac came in 5 dazzling new colors: Blueberry, Strawberry, Lime, Tangerine and Grape. Essentially a speed-bump of the original iMac, the Rev. C lacked both the mysterious "mezzanine" slot and the IRDA port, which lowered its price to $1199. The Rev. C was replaced just a few months later by the iMac Rev. D.

Picture Credits:
Apple, Inc.