apple-history.com / Macintosh SE FDHD

apple-history / Macintosh SE FDHD

# Macintosh SE FDHD

Essentials

Family: Classic Macs

Codename: Mac ±, PlusPlus, Aladdin, Freeport, Maui, Chablis

Gestalt ID: 5

Minimum OS: System 3.0/Finder 5.1

Maximum OS: 7.5.5

Introduced: August 1989

Terminated: October 1990

Processor

CPU: Motorola MC68000

CPU Speed: 8 MHz

FPU: none

Bus Speed: 8 MHz

Register Width: 32-bit

Data Bus Width: 16-bit

Address Bus Width: 32-bit

ROM: 256 kB

RAM Type: 30 pin SIMM

Minimum RAM Speed: 150 ns

Onboard RAM: 0 MB

RAM slots: 4

Maximum RAM: 4 MB

Expansion Slots: 1 SE PDS

Video

Monitor: 9" built-in

Max Resolution: 1 bit 512x342

Storage

Hard Drive: 40 MB

Floppy Drive: 1 3.25" 1.4 MB SuperDrive

Input/Output

ADB: 2

Floppy: DB-19

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: mono 8 bit mini

Speaker: mono

Miscellaneous

Power: 100 Watts

Dimensions: 13.6" H x 9.69" W x 10.9" D

Weight: 17 lbs.

Introduced in August 1989, The SE FDHD was an update to the SE. It added a single 1.4 MB floppy drive and standardized the previously optional 40 MB hard drive. The Mac SE FDHD was also sold with a 20 MB hard drive in Europe as the Mac SE 1/20. The price remained the same.Thanks to Eric Rasmussen For OS info.

Picture Credits:
Todo Apple Blog