apple-history.com / Power Macintosh 8200

apple-history / Power Macintosh 8200

# Power Macintosh 8200

Essentials

Family: PowerMac

Codename: ?

Gestalt ID: 108

Minimum OS: 7.5.3

Maximum OS: 9.1

Introduced: April 1996

Terminated: Mid 1997

Processor

CPU: PowerPC 601

CPU Speed: 100/120 MHz

FPU: integrated

Bus Speed: 40 MHz

Register Width: 32-bit

Data Bus Width: 64-bit

Address Bus Width: 32-bit

Level 1 Cache: 16 kB data, 16 kB instruction

Level 2 Cache: 256 km DIMM

ROM: 4 MB

RAM Type: 168 pin DIMM

Minimum RAM Speed: 70 ns

Onboard RAM: 0 MB

RAM slots: 4

Maximum RAM: 512 MB

Expansion Slots: 3 PCI

Video

VRAM: 2 MB (4 MB via 2 DIMM sockets)

Max Resolution: all resolutions supported

Video Out: DB-15

Storage

Hard Drive: 750 MB-1.2 GB

Floppy Drive: 1.4 MB SuperDrive

Optical Drive: 4x/8x CD-ROM

Input/Output

ADB: 1

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: stereo 16 bit mini

Audio In: stereo 16 bit mini

Speaker: mono

Networking

Ethernet: AAUI-15, 10Base-T

Miscellaneous

Power: 150 Watts

Dimensions: 14" H x 7.7" W x 15.75" D

Weight: 25 lbs.

The 8200 was a version of the 7200 in a tower case. All other specs are the same as the 7200. The 8200 Shipped only in Europe.

Picture Credits:
John Greenleigh/Flipside Studios