apple-history.com / Macintosh SE/30

apple-history / Macintosh SE/30

# Macintosh SE/30

Essentials

Family: Classic Macs

Codename: Green Jade, Fafnir

Gestalt ID: 9

Minimum OS: 6.0.3

Maximum OS: 7.5.5

Introduced: January 1989

Terminated: October 1990

Processor

CPU: Motorola MC68030

CPU Speed: 16 MHz

FPU: 68882

Bus Speed: 16 MHz

Register Width: 32-bit

Data Bus Width: 32-bit

Address Bus Width: 32-bit

Level 1 Cache: 256 bytes data, 256 bytes instruction

ROM: 256 kB

RAM Type: 30 pin SIMM

Minimum RAM Speed: 120 ns

Onboard RAM: 0 MB

RAM slots: 8

Maximum RAM: 32 MB

Expansion Slots: 1 SE/30 PDS

Video

Monitor: 9" built-in

Max Resolution: 1 bit 512x342

Storage

Hard Drive: 40-80 MB

Floppy Drive: 1.4 MB SuperDrive

Input/Output

ADB: 2

Floppy: DB-19

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: stereo 8 bit mini

Speaker: mono

Miscellaneous

Power: 75 Watts

Dimensions: 13.6" H x 9.6" W x 10.9" D

Weight: 19.5 lbs.

Released in January of 1989, The SE/30 was essentially a IIx inside an SE case. The second floppy feature of the SE was no longer offered in the SE/30, in favor of a built-in hard drive. The machine sold for $4,369.

Picture Credits:
Todo Apple Blog