apple-history.com / iMac DV SE (Summer 2000)

apple-history / iMac DV SE (Summer 2000)

# iMac DV SE (Summer 2000)

Essentials

Family: iMac/eMac

Codename: ?

Gestalt ID: 406

Minimum OS: 9.0.4

Maximum OS: 10.4.11

Introduced: July 2000

Terminated: February 2001

Processor

CPU: PowerPC 750 "G3"

CPU Speed: 500 MHz

FPU: integrated

Bus Speed: 100 MHz

Register Width: 32-bit

Data Bus Width: 64-bit

Address Bus Width: 32-bit

Level 1 Cache: 32 kB data, 32 kB instruction

Level 2 Cache: 512 kB backside, 1:2

ROM: 1 MB ROM + 3 MB toolbox ROM loaded into RAM

RAM Type: PC100

Minimum RAM Speed: 100 MHz

Onboard RAM: 0 MB

RAM slots: 2

Maximum RAM: 1 GB

Video

Monitor: 15"

GPU: ATI RAGE 128 Pro

VRAM: 8 MB SGRAM

Max Resolution: 1024x768

Video Out: VGA (mirror only)

Storage

Hard Drive: 30 GB

ATA Bus: ATA-66

Optical Drive: 4x DVD-ROM

Input/Output

USB: 2

Firewire: 2

Audio Out: stereo 16 bit mini

Audio In: stereo 16 bit mini

Speaker: Harman Kardon Odissey

Microphone: mono

Networking

Modem: 56 kbps

Ethernet: 10/100Base-T

Wi-Fi: optional 802.11b

Miscellaneous

Power: 150 Watts

Dimensions: 15" H x 15" W x 17.1" D

Weight: 40 lbs.

Announced in July 2000, the iMac DV SE (Summer 2000) built on the runaway success of the iMac DV SE. The processor speed was raised to 500 MHz, the hard drive was more than doubled to 30 GB, and a new color option (Snow) was added.

The iMac DV SE 2000 shipped with 128 MB of RAM, a 56 kbps modem, Apple's Pro Mouse, was avaiable in either Graphite or Snow, and cost $1499.

Picture Credits:
Apple, Inc.