apple-history.com / Workgroup Server 9650

apple-history / Workgroup Server 9650
Follow @apple_history
Tweet

# Workgroup Server 9650

Essentials

Family: Servers

Codename: ?

Gestalt ID: 67

Minimum OS: 7.6.1

Maximum OS: 9.1

Introduced: April 1997

Terminated: Early 1998

Processor

CPU: PowerPC 604e

CPU Speed: 233/350 MHz

FPU: integrated

Bus Speed: 50 MHz

Register Width: 32-bit

Data Bus Width: 64-bit

Address Bus Width: 32-bit

Level 1 Cache: 32 kB data, 32 kB instruction

Level 2 Cache: 512 kB DIMM

ROM: 4 MB

RAM Type: 168 pin DIMM

Minimum RAM Speed: 70 ns

Onboard RAM: 0 MB

RAM slots: 12

Maximum RAM: 1526 MB

Expansion Slots: 6 PCI

Storage

Hard Drive: 4.0 GB 7200 RPM

Floppy Drive: 1.4 MB SuperDrive

Optical Drive: 12x CD-ROM

Input/Output

ADB: 1

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: stereo 16 bit mini

Audio In: stereo 16 bit mini

Speaker: mono

Networking

Ethernet: AAUI-15, 10Base-T

Miscellaneous

Power: 390 Watts

Dimensions: 17.3" H x 9.7" W x 17.3" D

Weight: 35 lbs.

Notes

The 350 MHz model used a "Mach 5" 604e, with a 1 MB Inline level 2 cache, a 24x CD-ROM, and dual 4 GB hard drives.

The Workgroup Server 9650 was based on the motherboard of the PowerMac 9600, and included bundled server software. It was "speed bumped" to a 350 MHz "Mach 5" 604e processor in late 1997.

Picture Credits:
John Greenleigh/Flipside Studios