apple-history.com / Macintosh Quadra 610

apple-history / Macintosh Quadra 610
Follow @apple_history
Tweet

# Macintosh Quadra 610

Essentials

Family: Macintosh Quadra

Codename: Speedbump 610

Gestalt ID: 53

Minimum OS: 7.0.1

Maximum OS: 8.1

Introduced: October 1993

Terminated: July 1994

Processor

CPU: Motorola MC68040

CPU Speed: 25 MHz

FPU: integrated

Bus Speed: 25 MHz

Register Width: 32-bit

Data Bus Width: 32-bit

Address Bus Width: 32-bit

Level 1 Cache: 4 kB data, 4 kB instruction

ROM: 1 MB

RAM Type: 72 pin SIMM

Minimum RAM Speed: 80 ns

Onboard RAM: 4 MB

RAM slots: 2

Maximum RAM: 68 MB

Expansion Slots: 1 7" NuBus or PDS

Video

VRAM: 512 kB - 1 MB (two sockets)

Max Resolution: 1152x870

Video Out: DB-15

Storage

Hard Drive: 80-500 MB

Floppy Drive: 1.4 MB SuperDrive

Optical Drive: 2x CD-ROM

Input/Output

ADB: 2

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: mono 8 bit mini

Audio In: stereo 8 bit mini

Speaker: mono

Microphone: mono

Networking

Ethernet: AAUI-15

Miscellaneous

Power: 210 Watts

Dimensions: 3.4" H x 16.3" W x 15.6" D

Weight: 14 lbs.

Introduced in October 1993, the Quadra 610 replaced the Centris 610, adding a 25 MHz 68040 processor. The price for the Quadra 610 remained $2,520.

Picture Credits:
Todo Apple Blog