apple-history.com / Newton Message Pad 100

apple-history / Newton Message Pad 100
Follow @apple_history
Tweet

# Newton Message Pad 100

Essentials

Family: Newton

Codename: Junior, Wedge

Minimum OS: Newton OS 1.2

Maximum OS: Newton OS 1.3

Introduced: March 1994

Terminated: April 1995

Processor

CPU: ARM 610

CPU Speed: 20 MHz

FPU: none

Register Width: 32-bit

Data Bus Width: 32-bit

Address Bus Width: 32-bit

Level 1 Cache: 4 kB

ROM: 4 MB

Onboard RAM: 640 kB

Maximum RAM: 640 kB

Expansion Slots: 1 Type II PCMCIA

Video

Screen: reflective LCD

Max Resolution: 1 bit 336x240

Input/Output

Serial: 1

Speaker: mono

Networking

Modem: 9600 bps, optional

Miscellaneous

Dimensions: 7.25" H x 4.50" W x 0.75" D

Weight: 0.9 lbs.

Announced in March 1994, The NMP 100's hardware was virtually identical to that of the original NMP. It included a new version of the Newton OS, however, which improved the handwriting-recognition somewhat and fixed a number of bugs. The price was also dropped to $499. The NMP 100 was discontinued in August 1995.

For much more about the Newton Message Pad 100, and all Newton devices, check out the Newton Gallery.

Picture Credits:
EveryMac.com