apple-history.com / Power Macintosh 4400

apple-history / Power Macintosh 4400
Follow @apple_history
Tweet

# Power Macintosh 4400

AKA

Performa 4400

Power Macintosh 7220

Essentials

Family: PowerMac

Codename: Cupid, Tanzania

Gestalt ID: 514

Minimum OS: 7.5.3

Maximum OS: 9.1

Introduced: November 1996

Terminated: February 1998

Processor

CPU: PowerPC 603e

CPU Speed: 150/200 MHz

FPU: integrated

Bus Speed: 40 MHz

Register Width: 32-bit

Data Bus Width: 64-bit

Address Bus Width: 32-bit

Level 1 Cache: 16 kB data, 16 kB instruction

ROM: 4 MB

RAM Type: 168 pin DIMM

Minimum RAM Speed: 70 ns

Onboard RAM: 0 MB

RAM slots: 3

Maximum RAM: 160 MB

Expansion Slots: 2 12" PCI, 1 7" PCI, comm II

Video

VRAM: 1 - 4 MB

Max Resolution: all resolutions supported

Video Out: DB-15

Storage

Hard Drive: 1.2 GB

Floppy Drive: 1.4 MB SuperDrive

Optical Drive: 8x CD-ROM

Input/Output

ADB: 1

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: stereo 16 bit mini

Audio In: stereo 16 bit mini

Speaker: mono

Networking

Ethernet: 10Base-T

Miscellaneous

Power: 150 Watts

Dimensions: 5.43" H x 15.12" W x 17.37" D

Weight: 24 lbs.

Notes

The Gestalt ID of the 200 MHz model was 515, and it shipped with a 12x CD-ROM, a 256 kB L2 cache, and a 2 GB hard drive.

Released in November 1996, the Performa 4400/160 shipped only in europe. It came in a newly designed low profile case, with the floppy drive on the left. (a Mac rarity) It had optional 256 kB L2 cache, and was bundled with either a 14, 15 or 17 inch monitor, keyboard, and mouse. The 4400 was released in the US in February 1997 as the Power Mac 4400, with a 200 MHz 603e. It was discontinued a year later. The 4400/200 was also released in Australia as the Power Mac 7220.

Picture Credits:
John Greenleigh/Flipside Studios