apple-history.com / Macintosh Server G3

apple-history / Macintosh Server G3
Follow @apple_history
Tweet

# Macintosh Server G3

Essentials

Family: Servers

Codename: ?

Gestalt ID: 510

Minimum OS: 8.0

Maximum OS: 10.2.8

Introduced: March 1998

Terminated: January 1999

Processor

CPU: PowerPC 750 "G3"

CPU Speed: 233/266/300/333 MHz

FPU: integrated

Bus Speed: 66 MHz

Register Width: 32-bit

Data Bus Width: 64-bit

Address Bus Width: 32-bit

Level 1 Cache: 32 kB data, 32 kB instruction

Level 2 Cache: 1 MB backside, 1:2

ROM: 4 MB

RAM Type: 168 pin DIMM

Minimum RAM Speed: 100 MHz

Onboard RAM: 0 MB

RAM slots: 3

Maximum RAM: 768 MB

Expansion Slots: 3 PCI, 1 personality (filled)

Video

VRAM: 2 - 6 MB (2 MB onboard, one socket)

Max Resolution: all resolutions supported

Video Out: DB-15

Storage

Hard Drive: dual 9 GB RAID

ATA Bus: EIDE

SCSI Bus: Ultra/Wide SCSI 3

Floppy Drive: 1.4 MB SuperDrive

Zip Drive: optional

Optical Drive: 24x CD-ROM

Input/Output

ADB: 1

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: stereo 16 bit mini

Audio In: stereo 16 bit mini

Speaker: mono

Networking

Ethernet: 10Base-T

Miscellaneous

Power: 240 Watts

Dimensions: 15.2" H x 9.6" W x 17.8" D

Weight: 33.1 lbs.

The Server G3 was based on the motherboard of the PowerMac G3, and included bundled server software, and a dual SCSI 9 GB internal RAID Hard Drive.

Picture Credits:
Apple, Inc.