apple-history.com / Workgroup Server 95

apple-history / Workgroup Server 95
Follow @apple_history
Tweet

# Workgroup Server 95

Essentials

Family: Servers

Codename: Menagerie, Chinook

Gestalt ID: 26

Minimum OS: A/UX 3.0.1

Introduced: March 1993

Terminated: April 1995

Processor

CPU: Motorola MC68040

CPU Speed: 33 MHz

FPU: integrated

Bus Speed: 33 MHz

Register Width: 32-bit

Data Bus Width: 32-bit

Address Bus Width: 32-bit

Level 1 Cache: 4 kB data, 4 kB instruction

ROM: 1 MB

RAM Type: 30 pin SIMM

Minimum RAM Speed: 80 ns

Onboard RAM: 0 MB

RAM slots: 16

Maximum RAM: 256 MB

Expansion Slots: 5 NuBus, 1 PDS

Video

VRAM: 1 MB - 2 MB (4 sockets)

Max Resolution: 1152x870

Video Out: DB-15

Storage

Hard Drive: 230 MB-1 GB

Floppy Drive: 1.4 MB SuperDrive

Optical Drive: 2x CD-ROM

Input/Output

ADB: 2

Serial: 2 Mini DIN-8

SCSI: DB-25

Audio Out: stereo 8 bit mini

Audio In: mono 8 bit mini

Speaker: mono

Networking

Ethernet: AAUI-15

Miscellaneous

Power: 303 Watts

Dimensions: 18.6" H x 8.9" W x 20.6" D

Weight: 36.8 lbs.

The Workgroup Server 95 was based on the Quadra 950 motherboard, and ran a special version of Unix.

Picture Credits:
Wikipedia